[1. Motor Type]
Select the “DYNASERV” for rotational motor and the “LINEARSERV” for linear motor.

[2. Input Voltage]
Select the main input voltage.

[3. Required Accuracy (Coin Width)]
Input the required accuracy.  This is used to calculate benchmark time for settling time.
By clicking “Input Support” button, a sub-window is displayed to calculate angle from the length.

[4. Inertia/Mass]
Input the load mass for the LINEARSERV.
Input inertia moment of the load for the DYNASERV.
For unknown inertia value, click “Inertia Cal.” button and calculate the inertial value.

[5. Moving Distance]
Input the moving distance.

[6. Vel/Tor Limits]
By clicking “detail” button, set the detailed parameters if you like to set the feeding velocity, there is an external torque, or input pulse rate is restricted in pulse string control.

[7. Narrow Selection]
Click “Narrow Selection” button and input the conditions if you like to narrow motor sizes and required accuracy.

[8. Select Motors]
By clicking “Execution” button, sizing result is displayed.
By clicking motor type in the list, motion profile and detailed information of the motor are displayed.