[1. Motion Profile Display]
By clicking a motor in the list, the motion profile, specifications and sizing conditions of the selected motor is displayed.
Acceleration time/Deceleration time: Time to reach feeding velocity
Moving Time: Time from motion command is executed till ended
Total Time: Time for Travel Time plus settling time
Load Ratio: Ratio of load inertia (load mass for the LINEARSERV) against rotor inertia (slider mass for the LINEARSERV) of motor
Cycle Time Restriction: Benchmark allowable continuous operation time for over load error in case of repetitive operation

[2. Change Moving Time]
By clicking “Moving Time [s]” in the list, sizing results are changed in order of shorter travel time.

[3. Print]
By clicking “Print” button, sizing result can be printed.
(in a language selected when executing the software)

[4. Save/Open]
It is able to save the sizing conditions and result.
The data is saved as tab paragraph format, and easily modified by Windows Excel and other applications.
(in a language selected when executing the software)