[Feeding Velocity]
Input feeding velocity if it is fixed.
If no assignment, rated speed is considered as the feeding velocity.

[Restricted Pulse Rate]
Check box, and input pulse restriction and commanded resolution in case of a pulse string control from PLC.
Restricted Pulse Rate: Input smaller value from maximum output pulse rate of PLC or maximum pulse rate of DrvG3.  Available pulse rate for DrvG3 is 2,000,000[pps] for differential interface, or interface must be open-collector.
Commanded Resolution: Input commanded resolution of 1 turn of motor for the DYNASERV.
                    Input commanded resolution of 1 meter move for the LINEARSERV.

[External Torque]
Input if there is a external torque toward rotating direction (besides motor friction).
If no assignment, sizing is performed on the condition of no external torque.