[1. Selection of Load Shape]
Select load shape.
If there is no applicable shape in the selection, divide into several sections and calculate by putting together those shapes.

[2. Material/Mass/Gravity]
Input load’s material, mass or gravity.
Input mass if “Mass” is selected.
Input gravity if “Gravity” is selected.

[3. Dimensions]
Input dimensions of load.  Input error influences the calculation result since inertia is in proportion to squared value of distance from central axis.
Input items are depending on what is selected in [2. Material/Mass/Gravity].  Input this section after completion of [2. Material/Mass/Gravity].

[4. Comment Input]
You can input ID, name or any information on the load.

[5. Others]
Modification: Input detail of the load can be modified by selecting the load # or clicking the load in list.
Deletion: Input data can be deleted by selecting the load # or clicking the load in list.